# EFI / The Boot Process

## What EFI is

**UEFI** (Unified Extensible Firmware Interface) is the software baked into your
machine's flash chip that runs the instant it powers on — the modern successor
to the legacy BIOS. Its job is to bring the hardware up to a sane state and then
find and launch an operating system. From our point of view it's a small runtime
that hands us a working CPU, a memory map, and a screen, and then gets out of the
way.

The key thing to understand: **UEFI is not our OS, it's a stepping stone.** It
exists to load *us*. Our `boot/efi.zig` is a UEFI *application* — a normal program
that the firmware runs — and its entire purpose is to gather what the kernel needs
and then jump into the kernel.

## How the firmware finds us

UEFI boots by looking for a FAT-formatted partition called the **EFI System
Partition (ESP)** and running a file at a well-known fallback path:

```
EFI/BOOT/BOOTX64.efi         <- the "removable media" default for x86-64
```

The boot volume is **FHS-shaped** (see the repository-layout note in
[README.md](../README.md)): the root `build.zig` compiles `boot/efi.zig` (built
for the `uefi` target) and `build/images.zig` places it at
`EFI/BOOT/BOOTX64.efi` — the one path UEFI firmware fixes — and lays
the rest out by FHS path: the kernel at `system/kernel`, init at
`system/services/init`, the pre-packed boot capsule at `boot/system.img`
([system-image.md](system-image.md)).
`zig-out` mirrors that tree, but what a machine actually boots is the
self-contained FAT32 image `tools/make-fat-image.py` builds from the same files
(`danos-usb.img`). The `run-x86-64` step points QEMU at OVMF (UEFI firmware for
virtual machines) and attaches that image (its serial-logging twin, built the
same way) as a USB mass-storage device on the xHCI bus — the guest never sees
`zig-out`. The firmware finds `BOOTX64.efi` on the image and runs it — that's
our `main()`, which then loads the kernel and the system binaries from their
FHS paths.

## Boot services: the firmware's API

While a UEFI app runs, it has access to **boot services** — a table of function
pointers the firmware provides for allocating memory, reading files, locating
hardware protocols, and so on. In `boot()` this is the very first thing we grab:

```zig
const bs = uefi.system_table.boot_services orelse return error.NoBootServices;
```

Everything the firmware offers hangs off tables reachable from
`uefi.system_table`: `boot_services`, `con_out` (the text console we `log()` to),
and the various *protocols* (GOP for graphics, SimpleFileSystem for disk access).

**The critical rule:** boot services are *temporary*. They stop existing the
moment we call `ExitBootServices`. So the loader's structure is dictated by one
constraint — **gather everything the kernel could ever need first, then exit.**
The comment in `boot()` says exactly this:

> Everything the kernel needs must be gathered *before* we exit boot services,
> since afterwards none of these calls are usable.

## What our loader actually does

The four milestones below are the spine of `boot()`. Along the way it also
captures the **ACPI RSDP** from the UEFI configuration table (while boot
services are still up), loads the system binaries into an in-RAM
**initial ramdisk** (`loadSystemTree` — normally a single read of the pre-packed
`boot\system.img` capsule, which already *is* the ramdisk wire format; it falls
back to opening each manifest-listed path, and walks the `/system` and `/test`
trees only as a last resort for hand-assembled sticks — the capsule's format, builder, and
fallback chain are documented in [system-image.md](system-image.md). Best-effort either way — a kernel-only
volume still boots), and builds the **bootstrap page tables** the kernel starts
life on (`buildBootstrapTables`), all before the jump:

### 1. Query the framebuffer (`queryFramebuffer`)

We ask the firmware for the **Graphics Output Protocol (GOP)**, which describes
the linear framebuffer — its address, resolution, pitch, and pixel format —
and, when we can, switch the display to its native resolution first:

- Locate GOP via its *handle* (not `locateProtocol`), because the same handle
  also carries the display's **EDID**.
- Read the EDID (trying the `EDID_ACTIVE` then `EDID_DISCOVERED` protocol on each
  GOP handle) and parse the first Detailed Timing Descriptor — by convention the
  panel's preferred (native) resolution. This is best-effort: firmware installs
  these protocols inconsistently, and OVMF with QEMU's stdvga doesn't expose them
  at all.
- If we got a native resolution, enumerate the GOP modes with `queryMode` and
  `setMode` to the one that matches it (must be a linear 32bpp layout we can
  paint into). If EDID gave us nothing, we **keep the firmware's current default
  mode** rather than guess — with a valid EDID the firmware normally defaults to
  the native mode itself, so its choice beats second-guessing it with, say, the
  largest advertised mode.
- Copy the resulting address/resolution/pitch/format into our own `Framebuffer`.

All of this *must* happen now, because after exit there's no GOP to ask. (See
[framebuffer.md](framebuffer.md) for what those fields mean.)

### 2. Load the kernel (`loadKernel` + `loadElf`)

- Use the **LoadedImage** protocol to discover which device we booted from, then
  **SimpleFileSystem** to open that volume.
- Open the kernel ELF at its FHS path (`system\kernel`), seek to the end to learn its
  size, rewind, and read the whole ELF into a firmware-allocated pool buffer. (`read`
  may return short, so we loop.)
- Parse the ELF: validate the `\x7fELF` magic and the `x86_64` machine type, then
  walk the program headers. For every `PT_LOAD` segment we:
  - reserve the exact physical pages it asks to be loaded at (`p_paddr`) via
    `allocatePages`,
  - `@memcpy` the file-backed bytes to that address,
  - `@memset` the `.bss` tail (the part where `p_memsz > p_filesz`) to zero.

The kernel is linked to *run* in the higher half (virtual base
`0xFFFFFFFF80000000`; `exe.image_base` in `build.zig` is the *virtual* address
`0xFFFFFFFF80100000`) but is *loaded* low: the linker script's `AT()` clauses
give every segment a low physical load address (`p_paddr`, with `.text` at
`0x100000`, 1 MiB), which is what the loader allocates and copies into. The
bootstrap page tables built before the jump map the high link addresses onto
those low physical pages. If a segment's `p_paddr` collided with
firmware-reserved memory, `allocatePages` would fail and we'd need to move the
load addresses.

`loadElf` returns `e_entry`, the kernel's entry-point address.

### 3. Exit boot services (`exitBootServices`)

This is the handoff's trickiest step. To exit, the firmware demands the current
**memory map** and its *key* — proof that we've seen the latest state of memory.
But allocating the buffer to hold the memory map can itself *change* the map,
invalidating the key. So it's a retry loop:

```
get map info -> allocate buffer (+ spare descriptors) -> get map
             -> try exit with map.key
             -> if it failed, the map moved: free, retry
```

Once `exitBootServices` succeeds, **the firmware's services are gone for good** —
we must never touch `bs`, `con_out`, or any protocol again. The machine is now
entirely ours.

### 4. Jump to the kernel

```zig
handoff(cr3, entry, &boot_information);
```

`handoff` is a single inline-asm block — `cli`, load the bootstrap page tables'
`cr3`, place the `boot_information` pointer in RDI, then `callq *entry` — so
nothing runs between the CR3 load and the jump. This never returns.

## The ABI subtlety: RCX vs RDI

There's a deliberate detail worth calling out. A UEFI binary is compiled with the
**Microsoft x64** calling convention (first argument in register **RCX**). Our
kernel is freestanding and uses the **SysV AMD64** convention (first argument in
**RDI**). If we let each side use its target's default, the loader would place
`boot_information` in RCX while the kernel looked for it in RDI — and the kernel
would read garbage.

So the convention is pinned explicitly to SysV via the shared
`boot_handoff.kernel_abi` (defined in `system/boot-handoff.zig`). The kernel's
`kmainEntry` declares `callconv(kernel_abi)`; the loader honours the same contract
by loading RDI by hand in `handoff`'s inline asm rather than trusting its own
Microsoft-x64 default. `kernel_abi` lives in the shared `boot-handoff` module
because it's a contract both binaries must agree on. See
[sysv.md](sysv.md) for what "SysV" means and where else it shows up.

## The handoff contract

The loader and kernel are two *separate* binaries built for two different targets,
so everything they exchange must have an identically-defined memory layout. That's
what `system/boot-handoff.zig` provides — imported by both as the `boot-handoff` module.
It is *only* the handoff: the kernel↔user ABI (`system/abi.zig`) and the device types
(`library/device/model/device-abi.zig`) are separate contracts the bootloader never sees.

- `BootInformation` — the top-level struct passed to the kernel: the
  framebuffer, the memory map, the kernel's own `PT_LOAD` segments
  (`kernel_segments` + `kernel_segment_count`, so the kernel can re-map itself
  with correct permissions), the ACPI RSDP address, and the initial-ramdisk
  base/length.
- `Framebuffer`, `PixelFormat`, `MemoryMap`/`MemoryRegion`, `KernelSegment`,
  `kernel_abi` — the shared field layouts and the calling convention.

The structs are `extern struct`, giving them a stable, C-compatible layout so the
bytes the loader writes are the bytes the kernel reads.

## The whole flow at a glance

```
power on
  -> UEFI firmware initialises hardware
  -> finds EFI/BOOT/BOOTX64.efi on the FHS volume, runs it   (our efi.zig main)
       -> grab boot services (+ the ACPI RSDP from the configuration table)
       -> queryFramebuffer   (via GOP: EDID native res, setMode, describe fb)
       -> loadKernel         (read system/kernel ELF, load PT_LOAD segments low, .text at 0x100000)
       -> loadSystemTree     (read the boot\system.img capsule as the in-RAM initial ramdisk;
                              fallbacks: manifest-listed paths, then a /system + /test tree walk)
       -> buildBootstrapTables (identity + physmap + higher-half kernel mappings)
       -> exitBootServices   (retry until the memory-map key holds)
       -> handoff: load bootstrap CR3, jump to e_entry, boot_information pointer in RDI
  -> kernel _start           (architecture/x86_64/isr.s: switch to a kernel-owned stack,
                              call kmainEntry -> paging, heap, device discovery,
                              scheduler, SMP, user space)
```

Bottom line: **UEFI's job is to give us a CPU, memory, and a framebuffer, then
disappear.** `boot/efi.zig` is the thin bridge that collects those gifts into a
`BootInformation`, tears down the firmware, and jumps into the kernel — after
which we're on our own.
